更新说明

注意：

1. 升级到V6.0后，RTP需要重新校准，并把灵敏度值从0x14改成0x40 。

如果从V6.0降级到TA指令集或V55，触摸屏一样要重新校准，但是灵敏度值不用修改。

（2）DGUS V6.0把TCON配置单独一个.INI文件来实现，需要额外下载。

（3）曲线自动读取变量数据，只需要升级OS核程序就可以，任何版本DGUS都支持。

Release Notes

Notes:

1. After upgrading to V6.0, RTP needs to be recalibrated, and the sensitivity value should be changed from 0x14 to 0x40.

If you downgrade from V6.0 to TA instruction set or V55, the touch screen also needs to be recalibrated, but the sensitivity value does not need to be modified.

(2) DGUS V6.0 implements TCON configuration with a single .INI file, which requires additional download.

(3) The curve automatically reads variable data, only need to upgrade the OS kernel program, any version of DGUS is supported.